**SOP - Framing 101** Logo, company name

Description automatically generated

Roof Truss



Electrical wires and plumbing run through the walls with small holes drilled in the studs and plates.

Stud – 16” on center (from center of 2 X 4 or 2 X 6 to center of next stud.

2 X 4 actually measure 1.5 X 3.5!

Header or Top Plate

Footer or Bottom Plate (Treated Lumber)



Windows are hung from the outside before the siding is applied, nailed into the studs.

All areas between the walls must be fire safe (sealed so no air gets in). Drywall seals the inside once installed.